			BOXES 
1.   15 Sheets -  ¾ inch   4x8 treated plywood 
2.  60 2x4x8 treated 2x4’s 
3. 6 pair heavy-duty hinges 
4. 12 latches  (6 inside/6 outside) 
5.  12 door handles 
6.  Concrete bases recommended (optional).   Boxes can sit on  
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Additional:  
Boxes must be white in color,  numbered 1 through 6 
Door is in the back of box with a latch & handle on the outside / latch and handle on the inside  
Air slots are on the sides-  6 inches long x ½ wide,  6 inches from the bottom  
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